IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition [CoordinationView]"
File name: "Project Number"
Time stamp: "2024-07-17T17:47:29"
Preprocessor: "The EXPRESS Data Manager Version 5.02.0100.07 : 28 Aug 2013"
Originating system: "20190725_1135(x64) - Exporter 20.1.0.81 - Default UI"
Application: "Autodesk Revit 2020 (ITA)" version "2020" identifier "Revit" by Organization "Autodesk Revit 2020 (ITA)"

People and organizations
  Person "nino.mazza@oneteam.it" of Organization (no name given)
  Owner history of Person "nino.mazza@oneteam.it" of Organization (no name given) | application "Autodesk Revit 2020 (ITA)" version "2020" identifier "Revit" by Organization "Autodesk Revit 2020 (ITA)" | change NOCHANGE | created 1721231248 (2024-07-17T15:47:28Z)

Units
  LENGTHUNIT: MILLI METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  PLANEANGLEUNIT: DEGREE (conversion based)
  MASSUNIT: KILO GRAM
  MASSDENSITYUNIT: derived
  TIMEUNIT: SECOND
  FREQUENCYUNIT: HERTZ
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  THERMALTRANSMITTANCEUNIT: derived
  VOLUMETRICFLOWRATEUNIT: derived
  ELECTRICCURRENTUNIT: AMPERE
  ELECTRICVOLTAGEUNIT: VOLT
  POWERUNIT: WATT
  FORCEUNIT: KILO NEWTON
  ILLUMINANCEUNIT: LUX
  LUMINOUSFLUXUNIT: LUMEN
  LUMINOUSINTENSITYUNIT: CANDELA
  USERDEFINED: derived "Luminous Efficacy"
  LINEARVELOCITYUNIT: derived
  PRESSUREUNIT: PASCAL
  USERDEFINED: derived "Friction Loss"

Spatial structure
IFCPROJECT "Project Number" | long name "Project Name" | phase "Project Status"
  IFCSITE "Default" | latitude 42° 21′ 31.181945″ | longitude -71° 3′ 24.263305″ | elevation above sea level 0.
    IFCBUILDING
      IFCBUILDINGSTOREY "Level 1" | long name "Level 1" | object type "Livello:8mm Head" | elevation 0.
        contains 1 element
          1 x IFCFLOWFITTING | type IFCPIPEFITTINGTYPE "Kit 3033677" | object type "3033677:Kit 3033677" | names: "3033677:Kit 3033677:206230" | material: materials ("150_150_150", "185_185_175", "Default", "250_160_0", "224_242_255", "165_132_0", "153_153_153") | property sets: Pset_DistributionFlowElementCommon, Pset_ManufacturerTypeInformation, Pset_QuantityTakeOff, Altro, Dimensioni, Fasi

Types
  IFCPIPEFITTINGTYPE "Kit 3033677" | 1 occurrence | material: materials ("150_150_150", "185_185_175", "Default", "250_160_0", "224_242_255", "165_132_0", "153_153_153") | property sets: Altro, Dati, Dati identità, Vincoli

Property sets
  Vincoli(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Base quota altimetrica = "Punto base progetto" (IFCIDENTIFIER)
  Grafica(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Colore = 0 (IFCINTEGER)
    Modello di linea = "Center" (IFCLABEL)
    Simbolo = "M_Level Head - Circle: M_Level Head - Circle" (IFCLABEL)
    Simbolo a estremità 1 per default = FALSE (IFCBOOLEAN)
    Simbolo a estremità 2 per default = TRUE (IFCBOOLEAN)
    Spessore di linea = "1" (IFCIDENTIFIER)
  Pset_DistributionFlowElementCommon | properties | on 1 object (1 IFCFLOWFITTING)
    Reference = "Kit 3033677" (IFCIDENTIFIER)
  Pset_ManufacturerTypeInformation | properties | on 1 object (1 IFCFLOWFITTING)
    Manufacturer = "Immergas" (IFCLABEL)
  Pset_QuantityTakeOff | properties | on 1 object (1 IFCFLOWFITTING)
    Reference = "Kit 3033677" (IFCIDENTIFIER)
  Altro | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    Categoria = "Informazioni sul progetto" (IFCLABEL)
    Data di consegna del progetto = "Issue Date" (IFCTEXT)
    Indirizzo del progetto = "## Street City, State Zip" (IFCTEXT)
    Nome del cliente = "Owner" (IFCTEXT)
    Nome del progetto = "Project Name" (IFCTEXT)
    Numero del progetto = "Project Number" (IFCTEXT)
    Stato del progetto = "Project Status" (IFCTEXT)
  Altro | properties | on 1 object (1 IFCFLOWFITTING)
    Categoria = "Raccordi tubazione" (IFCLABEL)
    Famiglia = "3033677: Kit 3033677" (IFCLABEL)
    Famiglia e tipo = "3033677: Kit 3033677" (IFCLABEL)
    ID tipo = "3033677: Kit 3033677" (IFCLABEL)
    Tipo = "3033677: Kit 3033677" (IFCLABEL)
  Altro | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Categoria = "Livelli" (IFCLABEL)
    Famiglia = "Livello: 8mm Head" (IFCLABEL)
    Famiglia e tipo = "Livello: 8mm Head" (IFCLABEL)
    ID tipo = "Livello: 8mm Head" (IFCLABEL)
    Tipo = "Livello: 8mm Head" (IFCLABEL)
  Altro | properties | on 1 type object
    Categoria = "Raccordi tubazione" (IFCLABEL)
    ETIM Note = "Residential heating" (IFCTEXT)
    MasterFormat = "32 00 00- Heating, Ventilating, and Air Conditioning (HVAC)" (IFCTEXT)
    Masterformat 2014 Description = "Heating, Ventilating, and Air Conditioning (HVAC)" (IFCTEXT)
    Nome famiglia = "3033677" (IFCTEXT)
    Omniclass Description = "HVAC Specific Products and Equipment" (IFCTEXT)
    Uniformat = "Heat Generating Systems" (IFCTEXT)
    Uniformat II Description = "Heat Generating Systems" (IFCTEXT)
    Uniformat code = "D3020" (IFCTEXT)
  Dimensioni | properties | on 1 object (1 IFCFLOWFITTING)
    Area = 0.418779377468845 (IFCAREAMEASURE) [SQUARE_METRE]
    Dimensioni = "" (IFCTEXT)
    Volume = 0.00715427815508101 (IFCVOLUMEMEASURE) [CUBIC_METRE]
  Dimensioni | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Altezza di calcolo = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Fasi | properties | on 1 object (1 IFCFLOWFITTING)
    Fase di creazione = "New Construction" (IFCLABEL)
  Isolamento | properties | on 1 object (1 IFCFLOWFITTING)
    Dimensione totale = "" (IFCTEXT)
    Spessore isolamento = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Meccanica | properties | on 1 object (1 IFCFLOWFITTING)
    Metodo di perdita = "3bf616f9-6b98-4a21-80ff-da1120c8f6d6" (IFCTEXT)
  Vincoli | properties | on 1 object (1 IFCFLOWFITTING)
    Quota altimetrica da livello = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Sposta con l'oggetto più vicino = FALSE (IFCBOOLEAN)
  Vincoli | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Quota altimetrica = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Vincoli | properties | on 1 type object
    Prospetto di default = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Dati identità | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    Autore = "" (IFCTEXT)
    Descrizione organizzazione = "" (IFCTEXT)
    Nome edificio = "" (IFCTEXT)
    Nome organizzazione = "" (IFCTEXT)
  Dati identità | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Nome = "Level 1" (IFCTEXT)
    Piano edificio = TRUE (IFCBOOLEAN)
    Strutturale = FALSE (IFCBOOLEAN)
  Dati identità | properties | on 1 type object
    Codice assieme = "" (IFCTEXT)
    Commenti sul tipo = "" (IFCTEXT)
    Descrizione assieme = "" (IFCTEXT)
    Manufacturer Product Link = "https://www.immergas.com/en/home_eng" (IFCTEXT)
    Modello = "" (IFCTEXT)
    Nome codice = "" (IFCTEXT)
    Nome del tipo = "Kit 3033677" (IFCTEXT)
    Numero OmniClass = "" (IFCTEXT)
    Produttore = "Immergas" (IFCTEXT)
    Titolo OmniClass = "" (IFCTEXT)
  Pset_BuildingStoreyCommon | properties | on 1 object (1 IFCBUILDINGSTOREY)
    AboveGround = UNKNOWN (IFCLOGICAL)
  Pset_BuildingCommon | properties | on 1 object (1 IFCBUILDING)
    IsLandmarked = UNKNOWN (IFCLOGICAL)
    NumberOfStoreys = 1 (IFCINTEGER)
  Altro(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Categoria = "Livelli" (IFCLABEL)
    Nome famiglia = "Livello" (IFCTEXT)
  Dati identità(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Nome del tipo = "8mm Head" (IFCTEXT)
  Dati | properties | on 1 type object
    Codice = "3.033676 3.03668 3.033677" (IFCTEXT)
    Description_en = "Plate heat exchanger kit for single installation on the right side of VICTRIX PRO 100/120/150/180 V2 The kit includes connecting pipes, air vent, discharge tap, filling taps and connection to expansion vessel" (IFCTEXT)
    Description_it = "Kit scambiatore a piastre per installazione singola lato destro VICTRIX PRO 100/120/150/180 V2 Comprensivo di tubi collegamento, sfiato aria, rubinetto di scarico, attacchi per riempimento e attacco vaso d’espansione (non fornito di serie). Piastre non smontabili e ispezionabili." (IFCTEXT)
    Foglio istruzioni = "https://www.immergas.com/media/Accessorio/6466166c0cda9aad94ba340e/1.047557.pdf" (IFCTEXT)
    Name_en = "Plate heat exchanger kit for single installation on the right side of VICTRIX PRO 100/120/150/180 V2" (IFCTEXT)
    Name_it = "Kit scambiatore a piastre per installazione singola lato destro VICTRIX PRO 100/120/150/180 V2" (IFCTEXT)

Other addresses and roles
  2 x postal address: "## Street City, State Zip", "Boston", "MA"