IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition [CoordinationView]"
File name: "Project Number"
Time stamp: "2019-12-20T09:12:19"
Preprocessor: "The EXPRESS Data Manager Version 5.02.0100.07 : 28 Aug 2013"
Originating system: "20181015_0930(x64) - Exporter 18.0.3.6 - Default UI"
Application: "Autodesk Revit 2018 (ITA)" version "2018" identifier "Revit" by Organization "Autodesk Revit 2018 (ITA)"

People and organizations
  Person "Traceparts" of Organization (no name given)
  Owner history of Person "Traceparts" of Organization (no name given) | application "Autodesk Revit 2018 (ITA)" version "2018" identifier "Revit" by Organization "Autodesk Revit 2018 (ITA)" | change NOCHANGE | created 0 (1970-01-01T00:00:00Z)

Units
  LENGTHUNIT: MILLI METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  PLANEANGLEUNIT: DEGREE (conversion based)
  MASSUNIT: KILO GRAM
  MASSDENSITYUNIT: derived
  TIMEUNIT: SECOND
  FREQUENCYUNIT: HERTZ
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  THERMALTRANSMITTANCEUNIT: derived
  VOLUMETRICFLOWRATEUNIT: derived
  ELECTRICCURRENTUNIT: AMPERE
  ELECTRICVOLTAGEUNIT: VOLT
  POWERUNIT: WATT
  FORCEUNIT: KILO NEWTON
  ILLUMINANCEUNIT: LUX
  LUMINOUSFLUXUNIT: LUMEN
  LUMINOUSINTENSITYUNIT: CANDELA
  USERDEFINED: derived "Luminous Efficacy"
  LINEARVELOCITYUNIT: derived
  PRESSUREUNIT: PASCAL
  USERDEFINED: derived "Friction Loss"

Spatial structure
IFCPROJECT "Project Number" | long name "Project Name" | phase "Project Status"
  IFCSITE "Default" | latitude 42° 21′ 31.181945″ | longitude -71° 3′ 24.263305″ | elevation above sea level 0.
    IFCBUILDING | postal address: "## Street City, State Zip", "Boston", "MA"
      IFCBUILDINGSTOREY "Level 1" | long name "Level 1" | elevation 0.
        contains 1 element
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Immergas-Ares pro 230" | object type "Immergas-Ares pro 230" | names: "Immergas-Ares pro 230:Immergas-Ares pro 230:202899" | material: materials ("Immergas - Plastica Nero", "Immergas - Alluminio") | property sets: Pset_BuildingElementProxyCommon, Pset_ManufacturerTypeInformation, Altro, Dati identità, Dimensioni, Fasi

Types
  IFCBUILDINGELEMENTPROXYTYPE "Immergas-Ares pro 230" | 1 occurrence | material: materials ("Immergas - Plastica Nero", "Immergas - Alluminio") | property sets: Altro, Costruzione, Dati identità, Dimensioni, Idraulica, Ingegneria elettrica

Property sets
  Vincoli(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Base quota altimetrica = "Punto base progetto" (IFCIDENTIFIER)
  Grafica(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Colore = 0 (IFCINTEGER)
    Modello di linea = "Center" (IFCLABEL)
    Simbolo = "M_Level Head - Circle: M_Level Head - Circle" (IFCLABEL)
    Simbolo a estremità 1 per default = FALSE (IFCBOOLEAN)
    Simbolo a estremità 2 per default = TRUE (IFCBOOLEAN)
    Spessore di linea = "1" (IFCIDENTIFIER)
  Pset_BuildingElementProxyCommon | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Reference = "Immergas-Ares pro 230" (IFCIDENTIFIER)
  Pset_ManufacturerTypeInformation | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Manufacturer = "Immergas" (IFCLABEL)
  Altro | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    Categoria = "Informazioni sul progetto" (IFCLABEL)
    Data di consegna del progetto = "Issue Date" (IFCTEXT)
    Indirizzo del progetto = "## Street City, State Zip" (IFCTEXT)
    Nome del cliente = "Owner" (IFCTEXT)
    Nome del progetto = "Project Name" (IFCTEXT)
    Numero del progetto = "Project Number" (IFCTEXT)
    Stato del progetto = "Project Status" (IFCTEXT)
  Altro | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Categoria = "Attrezzatura meccanica" (IFCLABEL)
    Famiglia = "Immergas-Ares pro 230: Immergas-Ares pro 230" (IFCLABEL)
    Famiglia e tipo = "Immergas-Ares pro 230: Immergas-Ares pro 230" (IFCLABEL)
    ID tipo = "Immergas-Ares pro 230: Immergas-Ares pro 230" (IFCLABEL)
    Tipo = "Immergas-Ares pro 230: Immergas-Ares pro 230" (IFCLABEL)
  Altro | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Categoria = "Livelli" (IFCLABEL)
    Famiglia = "Livello: 8mm Head" (IFCLABEL)
    Famiglia e tipo = "Livello: 8mm Head" (IFCLABEL)
    ID tipo = "Livello: 8mm Head" (IFCLABEL)
    Tipo = "Livello: 8mm Head" (IFCLABEL)
  Altro | properties | on 1 type object
    Categoria = "Attrezzatura meccanica" (IFCLABEL)
    ETIM Note = "Residential heating" (IFCTEXT)
    MasterFormat = "23 00 00- Heating, Ventilating, and Air Conditioning (HVAC)" (IFCTEXT)
    Masterformat 2014 Description = "Heating, Ventilating, and Air Conditioning (HVAC)" (IFCTEXT)
    Name BIM&CO = "Caldaia" (IFCTEXT)
    Nome famiglia = "Immergas-Ares pro 230" (IFCTEXT)
    Omniclass Description = "HVAC Specific Products and Equipment" (IFCTEXT)
    Operating Temperature = 90. (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
    Thermal power 80/60°C = 209290. (IFCPOWERMEASURE) [WATT]
    UDP_334_495_PORTATA_TERMICA = "214" (IFCTEXT)
    UDP_88_494_GAS_CONNECTION_DIAMETER = "0.75" (IFCTEXT)
    Uniformat = "Heat Generating Systems" (IFCTEXT)
    Uniformat II Description = "Heat Generating Systems" (IFCTEXT)
    Uniformat code = "D3020" (IFCTEXT)
  Dati identità | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    Autore = "" (IFCTEXT)
    Descrizione organizzazione = "" (IFCTEXT)
    Nome edificio = "" (IFCTEXT)
    Nome organizzazione = "" (IFCTEXT)
  Dati identità | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Contrassegno = "1" (IFCTEXT)
  Dati identità | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Nome = "Level 1" (IFCTEXT)
    Piano edificio = TRUE (IFCBOOLEAN)
    Strutturale = FALSE (IFCBOOLEAN)
  Dati identità | properties | on 1 type object
    Codice assieme = "" (IFCTEXT)
    Descrizione assieme = "" (IFCTEXT)
    Manufacturer Product Link = "https://www.immergas.com/en/product?title=ARES%20PRO%20230" (IFCTEXT)
    Modello = "Immergas-Ares pro 230" (IFCTEXT)
    Nome codice = "" (IFCTEXT)
    Nome del tipo = "Immergas-Ares pro 230" (IFCTEXT)
    Numero OmniClass = "" (IFCTEXT)
    Product Code = "3.028310" (IFCTEXT)
    Produttore = "Immergas" (IFCTEXT)
    Titolo OmniClass = "" (IFCTEXT)
  Dimensioni | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Area = 10.6075653044445 (IFCAREAMEASURE) [SQUARE_METRE]
    Volume = 1.44686709152574 (IFCVOLUMEMEASURE) [CUBIC_METRE]
  Dimensioni | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Altezza di calcolo = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Dimensioni | properties | on 1 type object
    Diameter of fume exhaust = 250. (IFCLENGTHMEASURE) [MILLI METRE]
    Overall Depth = 1082. (IFCLENGTHMEASURE) [MILLI METRE]
    Overall Height = 1917. (IFCLENGTHMEASURE) [MILLI METRE]
    Overall Width = 846. (IFCLENGTHMEASURE) [MILLI METRE]
  Fasi | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Fase di creazione = "New Construction" (IFCLABEL)
  Meccanica | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Classificazione sistema = "Altro,Mandata di sistema idronico,Ritorno di sistema idronico,Ventilazione,Altro,Comunicazione" (IFCTEXT)
    Nome sistema = "" (IFCTEXT)
  Meccanica | properties | on 1 type object
    Classificazione = "Nessuno" (IFCIDENTIFIER)
    Hydraulic Fittings = 1651. (IFCLENGTHMEASURE) [MILLI METRE]
    Piping volume boiler = 0.21 (IFCVOLUMEMEASURE) [CUBIC_METRE]
  Vincoli | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Host = "Nessuno" (IFCTEXT)
    Offset = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Vincoli | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Quota altimetrica = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Pset_BuildingStoreyCommon | properties | on 1 object (1 IFCBUILDINGSTOREY)
    AboveGround = UNKNOWN (IFCLOGICAL)
  Pset_BuildingCommon | properties | on 1 object (1 IFCBUILDING)
    NumberOfStoreys = 1 (IFCINTEGER)
  Altro(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Categoria = "Livelli" (IFCLABEL)
    Nome famiglia = "Livello" (IFCTEXT)
  Dati identità(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Nome del tipo = "8mm Head" (IFCTEXT)
  Costruzione | properties | on 1 type object
    Mass = 479. (IFCREAL)
    yield hvac heating load nominal (%) = 97.8 (IFCREAL)
    yield hvac heating load nominal 30 (%) = 96.5 (IFCREAL)
  Idraulica | properties | on 1 type object
    Dimensions of Piping Connectors = 19.05 (IFCLENGTHMEASURE) [MILLI METRE]
    Hot water flow = 0. (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
  Ingegneria elettrica | properties | on 1 type object
    Electric Power = 2098.9625312584 (IFCREAL)
    Frequency of use = 50. (IFCFREQUENCYMEASURE) [HERTZ]
    Nominal Current = 6. (IFCELECTRICCURRENTMEASURE) [AMPERE]
    Nominal Voltage = 230. (IFCELECTRICVOLTAGEMEASURE) [VOLT]
  Materiali e finiture | properties | on 1 type object
    Case = "Immergas - Alluminio" (IFCLABEL)
    cerniere = "Immergas - Plastica Nero" (IFCLABEL)